i) Description: 
The Elevation and Azimuth signals of a Sennheiser TCC2 ceiling microphone are assign to predefined Zones and activate corresponding camera presets of Panasonic AWHx-nn cameras. Four adjustable parameters take care of a smooth camera movement.

ii) Models:
The example program runs with Sennheiser TCC2 ceiling microphone and Panasonic AWHx-nn cameras. The module itself can be used to control  any devices.

iii) Manufacturer:
Does not apply

iv) Device Category:
Conferencing